{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["附件1","附件2","附件3","附件4","附件5"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"附件1","index":0,"n_rows":11,"n_cols":3,"rows_kept":11,"merged":[[0,0,0,2],[1,0,1,2]],"flags":["formulas_cached_only"]}
["附件1"]
["生产过程质量控制不严预警比例较高的8家预拌混凝土企业"]
["序号","企业名称"," 存在主要问题"]
[1,"长泰龙缘混凝土有限公司","掺合料罐体更换成水泥未报备，造成大量水泥投料出现负偏差警示，生产数据预警比例排名全省第一。"]
[2,"建宁县汉邦建材有限公司","出现较大量的投料正偏差预警，生产数据预警比例排名全省第二。"]
[3,"永安市永福混凝土工程有限公司","生产数据存在设计配合比编号无法匹配、生产配合比和设计配合比中胶凝材料用量不一致、实际投料量偏差超过规范要求等预警，生产数据预警比例排名全省第三。"]
[5,"志品（福州）技术工程有限公司","因生产前未向检测监管系统上传水泥、掺合料、砂、石、外加剂等原材料检验报告和设计配合比报告等原因出现预警，生产信息登记预警比例排名全省第一。"]
[4,"厦门固德建材有限公司","因生产前未向检测监管系统上传水泥、掺合料、砂、石、外加剂等原材料检验报告和设计配合比报告等原因出现预警，生产信息登记预警比例排名全省第二。"]
[5,"福州建迪混凝土有限公司","因生产前未向检测监管系统上传水泥、掺合料、砂、石、外加剂等原材料检验报告和设计配合比报告等原因出现预警，生产信息登记预警比例排名全省第三。"]
[7,"长泰龙缘混凝土有限公司","掺合料罐体更换成水泥未报备，造成大量水泥投料出现负偏差警示，胶凝材料投料负偏差比例超过10%，排名全省第一。"]
[8,"福建品胜混凝土有限公司","胶凝材料投料负偏差比例超过10%，排名全省第二。"]

{"sheet":"附件2","index":1,"n_rows":10,"n_cols":5,"rows_kept":10,"merged":[[0,0,0,4],[2,0,2,4]],"flags":["formulas_cached_only"]}
["附件2"]
[]
["检测失误造成检测结论错误的5家预拌混凝土企业"]
[]
["序号","企业名称","检测项目","报告编号","造成检测结论错误的原因"]
[1,"福建鸿东混凝土有限公司","水泥强度检验","HDN11600133","将普通硅酸盐水泥PO42.5R输成PO52.5，导致结论不准确。"]
[2,"连江县三强建材有限公司","水泥终凝时间","YZLN11600087","达到终凝状态的时间录入错误，造成终凝时间结论错误。"]
[3,"福建国柱混凝土有限公司","水泥烧失量","GZZ71600168","试样质量录入错误，将试样质量1g,录成试样质量+坩埚的质量37.848g，导致烧失量结论不准确。"]
[4,"华润混凝土（晋江）有限公司","水泥初凝时间和终凝时间","SZ71600017","达到初凝时间和终凝时间录入错误，造成初凝时间和终凝时间结论错误。"]
[5,"福建云信混凝土有限公司","水泥初凝时间","YZLN11600075","达到初凝状态的时间录入错误，造成初凝时间结论错误。"]

{"sheet":"附件3","index":2,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[0,0,0,4],[2,0,2,4]],"flags":["formulas_cached_only"]}
["附件3"]
[]
["检测失误造成检测结论错误的1家检测机构"]
[]
["序号","企业名称","检测项目","报告编号","造成检测结论错误的原因"]
[1,"连城县建设工程质量安全监督站","电渣压力焊\n拉伸试验","RZ31600684","收样人员录入样品信息时将公称直径20录成直径22，导致结论不准确。"]

{"sheet":"附件4","index":3,"n_rows":7,"n_cols":5,"rows_kept":7,"merged":[[0,0,0,4],[2,0,2,4],[5,0,6,0],[5,1,6,1],[5,2,6,2]],"flags":["formulas_cached_only"]}
["附件4"]
[]
["检测失误造成检测结论错误的1家施工企业试验室"]
[]
["序号","企业名称","检测项目","报告编号","造成检测结论错误的原因"]
[1,"中交三公局（北京）工程试验检测有限公司福州地铁二号线项目中心试验室","电弧焊拉伸试验","SJSYH11600453","试验人员误将待检区直径为18的钢筋电弧焊样品（编号H 11600596）当成是该样品直径20（编号H11600586）的钢筋电弧焊样品进行试验，导致结论不准确。"]
[{"$nulls":3},"SJSYH11600454","试验人员误将待检区直径为18的钢筋电弧焊样品（编号H 11600595）当成是该样品直径20（编号H11600582）的钢筋电弧焊样品进行试验，导致结论不准确。"]

{"sheet":"附件5","index":4,"n_rows":17,"n_cols":3,"rows_kept":17,"merged":[[2,0,2,2],[5,1,12,1],[13,1,14,1]],"flags":["formulas_cached_only"]}
["附件5"]
[]
["2016年度全年未被动态考核抽查抽测的\n预拌混凝土企业"]
[]
["序号","设区市","企业名称"]
[1,"福州市","福州吉成建材有限公司"]
[2,null,"福建国庄混凝土有限公司"]
[3,null,"福建国柱混凝土有限公司"]
[4,null,"福建建原混凝土有限公司"]
[5,null,"福州国泰混凝土有限公司"]
[6,null,"闽侯恒信混凝土有限公司晋安分公司"]
[7,null,"福建连江县丰源实业有限公司"]
[8,null,"福建龙资混凝土有限公司"]
[9,"莆田市","莆田市广汇混凝土有限公司"]
[10,null,"莆田市东风红混凝土有限公司"]
[11,"泉州市","泉州铭宇建设有限公司"]
[12,"漳州市","漳州市华信建材有限责任公司常山分公司"]